

|  |  |
| --- | --- |
|

|  |
| --- |
| **Baum Roll-By® mobile aneroid**Description* 300 mmHg clinical sphygmomanometer for mobile use.
* Meets the American National Standard ANSI/AAMI SP-10 for accuracy and performance.
* Available with Latex or Non-Latex components.
* Unique, low reflection, high contrast scale and red pointer to increase visibility and reduce parallax error.
* Diecast aluminum 5-wheel base(20”dia.) with 2”hooded casters and 2lb. cast iron weight for increased stability.
* Manometer housing is mounted at a 20° angle for ease of viewing.
* Heavy gauge machined aluminum tubing.
* Calibrated® V-Lok® inflation System and 8 feet of Extendex® coiled tubing.

Baum Roll-By® model 1150 - Large Basket* The Baum Roll-By® model 1150 has a large circular (360°) basket to store a full complement of inflation systems.

Finish:* Neutral White ABS plastic

Packaged Dimensions:* 22” L x 211⁄2” W x 151⁄4” H

Packaged Weight:* 17.70 lbs.

Standard Cuff Color:* Medium Blue

Cuff Size:* Adult

Inflation System:* Calibrated® V-Lok®

Cuff Holder:* Large Circular Basket
 |

 |
|  |