**MP-60A Syringe Pump**

1 9 infusion modes available: Rate, Time, Bodyweight, drip, sequential, trapezium, loading dose, micro, relay. ★

2 Infusion Rate Range: 0.1-1200ml/h, increment 0.1ml/h

3， VTBI Setting range 0.1-9999mL.

4， Infusion accuracy ≤±5%

5, KVO Rate: 0.1-5.0mL/h

6, Color TFT touch screen with screen auto lock★

7, 11 level occlusion available★

8, Anti Free-Flow design when opening the pump door★

9, Automatic door and Automatic anti-free-flow clamp★

10, Titration function available★

11, Calibration function to enable different brand syringe which is compliant to industry standard.

12, All types of alarm: Near End, Infusion End, Occlusion Alarm, Low Battery, Battery Empty, No Battery, No Power Supply, System trouble, Air Bubble and Reminder Alarm.

13, high sensitivity air bubble sensor with 7 levels choice★

14, Strong date storage: 2000 events can be stored★

15, Connectivity: LAN/WIFI function can connect to Infusion CMS★

16, Different mounting method, vertical or horizontal.

17 Long time battery support, up to 5 hours with 25ml/h infusion rate.

18 European CE or US FDA certification★

19 Very light design, only 1.2Kg with battery. ★

20 Barcode Scanner for quick patient information input★

21, 1.1 All set should be European CE/US FDA approved

22 Drop sensor specific mounting position should be available

23 Drug Library 1000 types★