**Goldway G40e**

* 12.1-inch color TFT LED display
* 800 X 600 pixels resolution
* Maximum display of 11 channels; auto channel height adjustment function
* Lightweight & ergonomic design
* Parameters: 3/5 lead ECG, HR, RESP, NBP, SpO2, PR, dual TEMP
* Optional dual IBP, etCO2 monitoring, and Cardiac Output function
* With ST segment analysis and 21 calls of arrhythmia
* FAST SpO2 technology with anti-motion and low perfusion performance
* Navigation wheel for information input and screen navigation
* Backlit function buttons for quick access to key functions
* Bed-to-bed overview function for up to 32 monitors without central monitoring system
* Bi-directional communication via LAN networking to a central monitoring system
* Standard HL7 output
* Fan-less design to reduce dust deposits
* Applications from neonate to adult
* With OxyCRG & minitrend
* With big number screen, dynamic trend screen, & OCRG screen
* 4 user-defined layout
* Timing clock configurable from 5-30mins
* 1,600 sets NBP table
* 1,200-hour trend graph of all parameters (with data manager function)
* 120-minute full disclosure ECG 1 waveform review (with data manager function)
* 200 sets alarm events & 200 sets arrhythmia events
* With drug calculation
* With HR variation & dynamic blood pressure analysis
* Rechargeable lithium ion battery with 2.5 hrs of operation
* Optional built-in 3-channel recorder
* Standard external interface available: ECG analog output, VGA output, Nurse call, LAN, USB
* Patient data export using a USB data manager
* Net weight: approximately 4.2kg