**MP-30A Syringe Pump**

* + 1. Automatic identify different size (5/10/20/30/50/60ml). ★
    2. 9 infusion modes: rate, time, bodyweight, trapezium, loading dose, sequential, micro, TIVA, relay★
    3. Infusion rate range: 0.1-2000mL/h, 0.1mL/h increment★
    4. Mechanical accuracy ±1%,accuracy including syringe ±2%★
    5. KVO available from 0.1-5.0mL/h
    6. 3 types of bolus available, manual bolus, rapid quantitative bolus, automatic bolus★

11 levels of alarm, low/middle/high alarm with audio and visual reminder

* + 1. Color TFT touch screen with screen auto lock★
    2. 11 level occlusion available★
    3. Titration function available★
    4. Calibration function to enable different brand syringe which is compliant to industry standard.
    5. All types of alarm: Near End, Infusion End, Occlusion Alarm, Low Battery, Battery Empty, No Battery, No Power Supply, System trouble, Air Bubble and Reminder Alarm.
    6. Strong date storage: 2000 events can be stored★
    7. Connectivity: LAN/WIFI function can connect to Infusion CMS★
    8. Long time battery support, up to 6 hours with 5ml/h infusion rate
    9. European CE or US FDA certification★
    10. Very light design, only 1.6Kg with battery. ★
    11. Barcode Scanner for quick patient information input★
    12. Drug Library 1000 types★