colro[**5**](http://www.wabaum.com/items.aspx?id=77)

**Baum Wall Aneroid (0950)**

|  |  |
| --- | --- |
|

|  |
| --- |
| Description* 300 mmHg swivel-type (110° arc) clinical sphygmomanometer for wall mounting.
* Meets the American National Standard ANSI/AAMI SP-10 for accuracy and performance.
* Available with Latex or Non-Latex components.
* Neutral White ABS plastic manometer with chrome plated steel bracket.
* Unique high contrast scale and red pointer increase visibility and reduce parallax error.
* 2 convenient cuff storage options available: large basket or small basket.
* Calibrated® V-Lok® inflation System with 8 feet of Extendex® Tubing.

Instrument Finish:* Neutral White ABS Plastic.

Instrument Dimensions:* 61⁄4” L x 61⁄4” W x 4” H

Packaged Dimensions:* 105⁄8” L x 71⁄4” W x 71⁄2” H

Basket Color:* Neutral White (standard)

Instrument Weight:* 1.10 lbs.

Packaged Weight:* 3.25 lbs

Cuff Size:* Adult

Inflation System:* Calibrated® V-Lok

Holder:* Wall Basket (Nylon Coated Steel)
 |

 |
|  |