**Technical Specifications:**

Brand: Philips

Model Name: PageWriter TC10

**ECG Function**

* Simultaneous lead acquisition (up to 12 leads)
* Can perform up to 6 channel rhythm strip
* 6 independent events can be marked for later review and analysis
* With five-minute full disclosure of up to 12 leads
* Up to 12 configured Exam Profiles can be specified
* With optional STEMI diagnostic aids (ST Maps, Critical Values, STEMI-CA) to support patient diagnosis
* ECG display is color coded to indicate lead signal quality
* With anatomical lead map that displays the location and label of loose or disconnected leads/electrodes
* Up to 20 lead reversal detection
* Capable of urgent/STAT ECG

**Physical features**

* Intuitive 1-2-3 operation for fast, efficient workflow
* 7” color touch screen display
* With buttons that light up to guide user
* Fully configurable patient ID fields
* On board “Help” for taking an ECG is available for main ECG functions
* With full screen preview of ECG waveforms to ensure high quality prior to printing
* 6 channel printer with PDF Wi-Fi/USB to external printer
* Printer paper size: 110 mm wide x 28.5 m long roll of thermal-sensitive paper
* Printing speed: 25, 50 mm/sec
* With removable li-on battery
* Battery capacity: 300 typical patient reports or 10 hours continuous operation without printing
* Local archive with maximum of 200 ECGs (PDF/XML file format)
* Transfer ECGs to USB memory stick (PDF/XML file format)
* Dimension: 338 mm x 240 mm x 65 mm
* Weight: 2.5 kg (5.5 lb)
* Capable of optional wireless LAN connection (802.11 a/b/g/n standards)
* Optional barcode reader
* With OPTIONAL five-minute full disclosure of up to 12 leads